SECTION 10 14 26

EXTERIOR SIGNAGE

Display hidden notes to specifier. (Don't know how? Click Here) 

** NOTE TO SPECIFIER ** Corpus Christi Stamp Works Inc. DBA/ National Signage Affiliates; . This section is based on the products of Corpus Christi Stamp Works Inc. DBA/ National Signage Affiliates, which is located at: P. O. Box 2189 502 S. Staples (78401) Corpus Christi, TX 78403 Toll Free: 800-322-4515 Fax: 800-354-6416 Email: sales@ccstampworks.com Web Site: www.ccswsignsystems.com 
1.	PART  1	  GENERAL
1.	1.1 		SECTION INCLUDES
** NOTE TO SPECIFIER ** Delete items below not required for project.
A.	A.		Exterior Signage Systems:
1.	1.		Building Identification Signage.
2.	2.		Directory and Directional Signage.
3.	3.		Post and Panel Signage.
4.	4.		Traffic Signage.
2.	1.2 		RELATED SECTIONS
** NOTE TO SPECIFIER ** Delete any sections below not relevant to this project; add others as required. 
A.	A.		Section 01100 – Administrative Requirements.
B.	B.		Section 09700 - Wall Finishes.
C.	C.		Section 10410 - Directories.
D.	D.		Section 16500 - Lighting.
2.	1.3 		REFERENCES
** NOTE TO SPECIFIER ** Delete references from the list below that are not actually required by the text of the edited section. 
A.	A.		Americans with Disabilities Act (ADA).
B.	B.		American National Standards Institute (ANSI):
1.	1.		ANSI A117.1 - Accessible and Usable Buildings and Facilities Standards.
2.	1.4 		SUBMITTALS
A.	A.		Submit under provisions of Section 01300.
B.	B.		Product Data: Manufacturer's data sheets on each product to be installed.
C.	C.		Shop Drawings: Shop drawings with letter style, dimensions, materials, finishes and general layout for each sign type, with sizes, edge and corner treatment, and mounting methods shown.
** NOTE TO SPECIFIER ** Delete if selection samples have already been selected.
A.	D.		Selection Samples: For each finish specified, two complete sets of color chips representing manufacturer's full range of available colors, patterns and finishes. 
** NOTE TO SPECIFIER ** Delete if verification sample not required.
A.	E.		Verification Samples: For each finish product specified, one full-size sign or typical letter representing actual product, color, patterns, and finishes. Include method of raised symbols and copy.
** NOTE TO SPECIFIER ** Delete if not required.
A.	F.	     Sustainable Design Submittals:
1.	1.	     Recycled Content – Provide documentation from Manufacturer verifying percentage of recycled and post-consumer content.
2.	2.	     Regional Materials – Provide documentation form manufacturer/distributor showing location where materials were obtained from for each component.
2.	1.5 		QUALITY ASSURANCE
A.	A.		Manufacturer Qualifications: Manufacturer shall have five years experience manufacturing and fabricating products of similar type and scope as those specified in this section.
** NOTE TO SPECIFIER ** Include a mock-up if the project size and/or quality warrant taking such a precaution. The following is one example of how a mock-up on a large project might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project. 
A.	B.		Regulatory Requirements:  Comply with applicable provisions in ADA-ABA Accessibility Guidelines, ICC/ANSI A117.1 and Unified Federal Accessibility Standards (UFAS)
B.	C.	    Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	1.		Finish areas designated by Architect.
2.	2.		Do not proceed with remaining work until workmanship, color, and sheen are approved by Architect.
3.	3.		Refinish mock-up area as required to produce acceptable work.
2.	1.6 		DELIVERY, STORAGE, AND HANDLING
A.	A.		Comply with manufacturer's recommendations for delivery, storage and handling.
B.	B.		Materials shall be delivered to the location in unopened, labeled factory containers. Upon delivery, materials shall be inspected for damage. Deficient materials shall not be used.
3.	1.7 		PROJECT CONDITIONS
A.	A.		Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
B.	PART  2	  PRODUCTS
4.	2.1 		MANUFACTURERS
A.	A.		Acceptable Manufacturer: Corpus Christi Stamp Works Inc. DBA/ National Signage Affiliates, which is located at: P. O. Box 2189 502 S. Staples (78401) ; Corpus Christi, TX 78403; Toll Free Tel: 800-322-4515; Email:  (sales@ccstampworks.com); Web: www.ccswsignsystems.com 
** NOTE TO SPECIFIER ** Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions. 
A.	B.		Substitutions: Not permitted.
B.	C.		Requests for substitutions will be considered in accordance with provisions of Section 01600.
** NOTE TO SPECIFIER ** Delete if not required. 
1.	2.2 		BUILDING IDENTIFICATION, DIRECTORY AND DIRECTIONAL SIGNAGE
** NOTE TO SPECIFIER ** Delete if not required. Delete options for model and size not required.
A.	A.		Subsurface Painted (SS)Series Signage: ADA compliant building identification signage system.
** NOTE TO SPECIFIER ** Delete options for model and associated text not required. 
1.	1.		Model: As indicated on Drawings.
2.	2.		Model: As selected by Architect.
3.	3.		Model: (Follow naming convention as described in catalog) SS-Sign Type-Graphic Process-Insert type (if needed)-Height- Width.
a.	a.	Description: ADA compliant sign with clear non-glare acrylic face with back painted/printed as specified and clear acrylic core; ADA text, pictograms chemically welded to face; DuraDot© Braille rasters as specified; Demarcation line – 1/32” high ADA approved plastic chemically welded to face, edges as specified.
b.	b.	Size: As indicated on Drawings; 
c.	c.	Size: As selected by Architect;
d.	d.	Size: __ inches (__ mm) in height  x __inches (__ mm) in width
3.	4.	Sign Face and Back
** NOTE TO SPECIFIER ** Delete options for number of colors/patterns per sign not required. 
a.	a.		Number of Colors/Patterns per Sign: As indicated on Drawings.
b.	b.	     Number of Colors/Patterns per Sign: As selected by Architect.
c.	c.	     Number of Colors/Patterns per Sign: ___color(s)/pattern(s).
d.	d.		Core Thickness: 1/8 inch (3 mm) or 1/4 inch (6 mm) thick per manufacturer recommendations.
** NOTE TO SPECIFIER ** Delete options for sign edges not required. 
5.	5.	Sign Edges: Matte.
6.	6.	Sign Edges: Polished.
** NOTE TO SPECIFIER ** Delete options/ paragraphs for room number panel not required. ** Select number of color options based on selection above. Fill in blanks with specific color/pattern designation, ' As indicated on Drawings' or ' As selected by Architect' as applicable. Delete options for color not required.
5.	7.	Room Number Panels: 1/8 inch (3 mm) thick clear non-glare acrylic.
a.	a.		Painted/ digitally printed Pattern/Colors: As indicated on Drawings.
b.	b.	     Painted/ digitally printed Pattern/Colors: As selected by Architect.
c.	c.	     Painted/ digitally printed Pattern/Colors:  ____.
6.	8.	Room Number Panels: (Luminous Subseries): Adhered to main sign panel in upper left corner, 1/2 inch (13 mm) thick acrylic.
a.	a.		Room Number Panel Color: As indicated on Drawings.
b.	b.		Room Number Panel Color: As selected by Architect.
c.	c.		Room Number Panel Color: _______________.
9.	9.		Main Sign Panels: 1/8 inch (3 mm) thick clear, non-glare acrylic.
a.	a.		Painted/ digitally-printed pattern/colors: As indicated on Drawings. 
b.	b.		Painted/ digitally-printed pattern/colors: As selected by Architect.
c.	c.		Painted/ digitally-printed pattern/colors: _______________.
** NOTE TO SPECIFIER ** Delete if not required. 
A.	B.		AlumaSet© (ALS) Series Signage: ADA compliant building identification signage system.
** NOTE TO SPECIFIER ** Delete options for materials and finish not required. 
1.	1.	Model No.: As indicated on Drawings.
2.	2.	Model No.: As selected by Architect.
3.	3.	Model No.: (Follow naming convention as described in catalog) ALS-Sign Type- Graphic Process-Insert type (if needed)- Height. Width.
a.	a.	     Description: ADA compliant sign with extruded aluminum frame. ADA text, pictograms topically applied to face; Changeable message inserts; DuraDot© Braille rasters as specified
b.	b.	     Size: As indicated on Drawings.
c.	c.	     Size: As selected by Architect.
d.	d.	     Size: __ inches (__ mm) in height  x __inches (__ mm) in width.
4.	4.	Extruded Aluminum Frame: Single Piece Extrusion
a.	a.	     Finish: As Indicated on Drawings.
b.	b.	     Finish: As Selected by Architect.
c.	c.	     Finish: Clear Anodized. 
d.	d.	     Finish: Painted.
5.	5.	Room Number Panel: Solid Aluminum Plate to Match Frame Finish.
6.	6.	Room Number Panel: Color Laminate on acrylic backing.
7.	7.	Room Name Panel: 3/16” Clear Non-Glare Acrylic lens.
8.	8.	Room Name Panel: Color Laminate on Acrylic Backing.
9.	9.	Room Name Panel: to match Aluminum Frame Finish.
10.	10.	Wayfinding/ Map Panel: Digitally printed graphic on Clear Non-Glare Acrylic Panel.
a.	a.	     Graphic as Indicated on Drawings.
b.	b.	     Owner/Architect to provide Graphic.
11.	11.	Message Inserts: Removable for copy changes, with set screw. Made of printed background with clear mylar insert.
a.	a.	     Painted/ digitally printed Pattern/Colors: As indicated on Drawings.
b.	b.	     Painted/ digitally printed Pattern/Colors: As selected by Architect.
c.	c.	     Painted/ digitally printed Pattern/Colors: __________.
d.	d.	     Text: Printed on clear mylar insert with color as indicated on Drawings.
e.	e.	     Text: Printed on clear mylar insert with color as selected by Architect.
f.	f.	      Text: Printed on clear mylar insert with color ____________.
** NOTE TO SPECIFIER ** Delete if not required. 
A.	C.		CS Series© Signage: ADA compliant building identification signage system.
** NOTE TO SPECIFIER ** Delete options for model and associated text not required. 
1.	1.		Model: As indicated on Drawings.
2.	2.		Model: As selected by Architect.
3.	3.	Model No.: (Follow naming convention as described in catalog) CS-Sign Type-Graphic Process-Insert type (if needed)- Height- Width.
a.	a.	     Description: ADA compliant sign with extruded aluminum frame. ADA text, pictograms chemically welded to face; Changeable message inserts; DuraDot© Braille rasters as specified
b.	b.	     Size: As indicated on Drawings.
c.	c.	     Size: As selected by Architect.
d.	d.	     Size: __ inches (__ mm) in height  x __inches (__ mm) in width.
3.	4.	Frame:  1/16 inch (1.5 mm) Aluminum Extrusion
a.	a.	    Finish: As selected by Architect.
b.	b.	    Finish: As indicated on Drawings.
c.	c.	    Finish: Satin Anodized.
d.	d.	    Finish: 312 Bronze Duranodic.
4.	5.	Sign Face 
** NOTE TO SPECIFIER ** Select face material and color/pattern designation. Fill in blanks with specific color/pattern designation (if needed), ' As indicated on Drawings' or ' As selected by Architect' as applicable. Delete options/paragraphs not required.
a.	a.	1/16 inch Clear Non-glare Acrylic Lens
b.	b.	1/16 inch Clear Non-glare Acrylic face with subsurface painted graphics.
c.	c.	1/8 inch Clear Non-glare Acrylic Lens.
d.	d.	1/8 inch Clear Non-glare Acrylic face with subsurface painted graphics.
e.	e.	1/4 inch Frosted Clear Acrylic.
f.	f.	1/4 inch Clear Acrylic with sub-surface painted background.
** NOTE TO SPECIFIER ** Delete options for core thickness not required. 
3.	6.	Core Thickness: 1/16 inch (1.5 mm) acrylic; 1/8 inch (3 mm) white acrylic; 1/8 inch (3mm) frosted clear acrylic; 1/4 inch (6 mm) frosted clear acrylic per manufacturer recommendation.
** NOTE TO SPECIFIER ** Delete options for sign edges not required. 
3.	7.	Sign Edges: Matte.
4.	8.	Sign Edges: Polished.
** NOTE TO SPECIFIER ** Delete options for subsurface graphics not required. 
3.	9.	Subsurface painted Pattern/Graphics/Colors: As indicated on Drawings.
4.	10.	Subsurface painted Pattern/Graphics/Colors: As selected by Architect.
5.	11.	Subsurface painted Pattern/Graphics/Colors: ____________.
** NOTE TO SPECIFIER ** Delete options for insert not required.
3.	12.		Insert: Printed vinyl on clear mylar.
a.	a.	     Lettering and graphics as indicated on Drawings.
b.	b.	     Lettering and graphics as selected by Architect.
** NOTE TO SPECIFIER ** Delete if not required. 
A.	D.		Lasered Acrylic (LA) Series Signage: ADA compliant building identification signage system.
** NOTE TO SPECIFIER ** Delete options for model and associated text not required. 
1.	1.		Model: As indicated on Drawings.
2.	2.		Model: As selected by Architect.
3.	3.	Model: (Follow naming convention as described in catalog) LA-Sign Type-Graphic Process-Insert type (if needed)- Height - Width.
1.	a.	Description: ADA compliant sign with clear non-glare acrylic face and frame each with back painted/printed as specified and clear acrylic core; ADA text, pictograms chemically welded to face; DuraDot© Braille rasters as specified; Edges as specified. Impervious to exterior weather conditions.  Also available with rastered graphics and subsurface text.
2.	b.	Size: As indicated on Drawings.
3.	c.	Size: As selected by Architect.
4.	d.	Size: __ inches (__ mm) in height  x __inches (__ mm) in width.
3.	4.	Frame:  Laser-Cut Acrylic: Subsurface painted and chemically welded to acrylic core
a.	a.	    Paint Color:  As Indicated on Drawings.
b.	b.	    Paint Color:  As selected by Architect.
c.	c.	    Paint Color:  ____________.
d.	d.	    Frame thickness: 1/4 inch
e.	e.	    Frame dimensions: As Indicated on Drawings.
f.	f.	     Frame dimensions: As selected by Architect.
g.	g.	    Frame dimensions: _________.
h.	h.	    Sign Edges: As indicated on Drawings.
i.	i.	     Sign Edges: As selected by Architect.
j.	j.	     Sign Edges: Matte.
k.	k.	    Sign Edges: Polished.
3.	5.	Core Panel:  1/8 inch (3 mm) or 1/4 inch (6 mm) thick per manufacturer recommendations.
4.	6.	Fixed Header Panel (select one)
a.	a.	    1/16 inch thick acrylic panel subsurface painted and chemically welded to acrylic core
1.	1)	    Raised Symbols: raised 1/32 inch (0.8 mm) from acrylic sign face, chemically welded to sign face.
2.	2)		Raised Lettering: 5/8 inch (16 mm) high minimum, raised 1/32 inch (0.8 mm), chemically welded to acrylic sign face.
3.	3)	     Lettering, numbering and symbols contrast with background,
** NOTE TO SPECIFIER ** Delete if not required. 
A.	E.		Spinnaker Series Signage: ADA compliant building identification signage system.
** NOTE TO SPECIFIER ** Delete options for model and associated text not required. 
1.	1.		Model: As indicated on Drawings.
2.	2.		Model: As selected by Architect.
3.	3.	(Follow naming convention as described in catalog). SP-Sign Type-Graphic Process-Insert type (if needed)- Height. Width.
a.	a.	     Description: ADA compliant sign with curved metal frame and either metal or acrylic endcaps; ADA text, pictograms topically applied; DuraDot© braille rasters as specified; Demarcation line – acrylic.
b.	b.	     Size: As indicated on Drawings.
c.	c.	     Size: As selected by Architect.
d.	d.	     Size: __ inches (__ mm) in height  x __inches (__ mm) in width.
** NOTE TO SPECIFIER ** Delete options for finish not required.
3.	4.	Frame:  Curved Aluminum Frame with Aluminum Endcaps.
4.	5.	Frame:  Curved Aluminum Frame with Acrylic Endcaps.
a.	a.	Finish: As indicated on Drawings.
b.	b.	Finish: As selected by Architect.
c.	c.	Finish: Satin Anodized.
d.	d.	Finish: Black.
e.	e.	Finish: Bronze.
f.	f.	Finish: _______.
3.	6.	Header Panel:
a.	a.	Polycarbonate Lens
      ** NOTE TO SPECIFIER ** Delete options for rasters, symbols and text not required. 
A.	F.	     Lettering, Numbering and Symbols
1.	1.	Braille: Tactile Grade 2 DuraDot© Braille integral with sign face, raised 1/32 inch (0.8 mm). 
a.	a.	Rasters: Acrylic rasters with .059 inch (1.5 mm) surface diameter, body of sphere pressure secured below face laminate. Glued-on dots are not acceptable.
1.	2.	VisiTouch® Raised Symbols: 3 inches (76 mm) high, raised 1/32 inch (0.8 mm) from sign face, chemically welded to acrylic or metal sign face.
a.	a.	Color:  As indicated on drawings.
b.	b.	Color:  As selected by Architect.
c.	c.	Color:  ________.
4.	4.	VisiTouch® Raised Lettering: 5/8 inch (16 mm) high minimum, raised 1/32 inch (0.8 mm) from sign face, topically applied to acrylic or metal sign face.
a.	a.	Color:  As indicated on drawings.
b.	b.	Color:  As selected by Architect.
c.	c.	Color:  ________.
d.	d.	 Lettering Style: As indicated on Drawings.
e.	e.	 Lettering Style: As selected by Architect.
f.	f.	 Lettering Style: Helvetica Medium, all upper case.
g.	g.	 Lettering Style: Helvetica Medium Condensed, all upper case.
4.	5.	VisiTouch® Raised Room Number: 5/8 inch (16 mm) high minimum, raised 1/32 inch (0.8 mm) from sign face, topically applied to acrylic or metal sign face.
a.	a.	Color:  As indicated on drawings.
b.	b.	Color:  As selected by Architect.
a.	b.	Color:  ________.
b.	c.	Lettering Style: As indicated on Drawings.
c.	d.	Lettering Style: As selected by Architect.
d.	e.	Lettering Style: Helvetica Medium, all upper case.
e.	f.	Lettering Style: Helvetica Medium Condensed, all upper case.
4.	6.	Copy: All Lettering, numbering and symbols contrast with background, eggshell matte finish.
** NOTE TO SPECIFIER ** Delete if not required.   Delete options for changeable message and text not required.
A.	G.	     Changeable Message Insert Panels:
1.	1.	Clear non-glare acrylic lens or window for engraved message insert
2.	2.	Acrylic Insert, Subsurface Painted
a.	a.	     Pattern/Graphics/Colors: To match sign face.
b.	b.	     Pattern/Graphics/Colors: as indicated on Drawings.
c.	c.	     Pattern/Graphics/Colors: as selected by Architect.
d.	d.	     Pattern/Graphics/Colors: ________.
e.	e.	     Text: As selected by Architect; 
f.	f.	     Text: As indicated on Drawings.
g.	g.	     Text: Topically applied vinyl.
h.	h.	     Text: Raised Lettering: 5/8 inch (16 mm) high minimum, raised 1/32 inch (0.8 mm) topically applied to sign face (ADA only).
i.	i.	     Lettering Style: As indicated on Drawings.
j.	j.	     Lettering Style: As selected by Architect.
k.	k.	    Lettering Style: Helvetica Medium, all upper case.
l.	l.	     Lettering Style: Helvetica Medium Condensed, all upper case.
m.	m.	    Braille: Raised tactile grade 2 Braille integral with sign face, raised 1/32 inch (0.8 mm). (ADA only.)
1.	1)	Rasters: Acrylic rasters with .059 inch (1.5 mm) surface diameters, body of sphere pressure secured below face laminate.
1.	3.	Clear Mylar Strip Insert:
a.	a.	     Text: As selected by Architect.
b.	b.	     Text: As indicated on Drawings.
c.	c.	     Text: Printed vinyl.
d.	d.	     Lettering Style: As indicated on Drawings.
e.	e.	     Lettering Style: As selected by Architect.
f.	f.	     Lettering Style: Helvetica Medium, all upper case.
g.	g.	     Lettering Style: Helvetica Medium Condensed, all upper case.
2.	4.	Message Insert to be provided by Owner
3.	5.	Magnetic Message Insert: Subsurface-painted Acrylic.
a.	a.	     1/16 inch thick acrylic panel subsurface painted with vinyl lettering reverse applied 
b.	b.	     1/16 inch thick acrylic panel subsurface painted with raised lettering  5/8 inch (16 mm) high minimum, raised 1/32 inch (0.8 mm), topically applied to sign face and Braille translation (ADA only.)
c.	c.	     Color: As selected by Architect.
d.	d.	     Color: As Indicated on Drawings.
e.	e.	     Color: to match sign face.
f.	f.	     Color: _________.
g.	g.	     Lettering Style: As indicated on Drawings.
h.	h.	     Lettering Style: As selected by Architect.
i.	i.	      Lettering Style: Helvetica Medium, all upper case.
j.	j.	      Lettering Style: Helvetica Medium Condensed, all upper case.
1.	2.3 		POST AND PANEL SIGNAGE
NOTE TO SPECIFIER ** Delete options for series and associated text not required.      
A.	A.	     BE Series Post and Panel Signage Systems: as manufactured by Corpus Christi Stamp Works Inc. DBA/ National Signage Affiliates.
1.	1.	     Model No: As indicated on Drawings.
2.	2.	     Model No: As selected by Architect.
3.	3.	     Model No: (Follow naming convention as described in catalog). BE - Post Type- Body Type - Panel Type - Sign Type - Graphic Process – Height – Width.
a.	a.	    	Description:  Non-illuminated Post and panel signage using Aluminum posts with single layer panels of either Dibond or Aluminum
b.	b.	     Size: As indicated on Drawings.
c.	c.	     Size: As selected by Architect.
d.	d.	     Size: __ inches (__ mm) in height  x __inches (__ mm) in width
1.	4.		Posts:  Aluminum
a.	a.		2 inch (51 mm) square posts, 
b.	b.		3 ¼” inch (83 mm) square posts
c.	c.	     3 ¼” inch (83mm) Diameter round posts
d.	d.	     Length/Height:  As Indicated on Drawings.
e.	e.	     Length/Height:  As Selected by Architect.
f.	f.	      Length/Height:  ____ inches.
g.	g.	     Finish:  Paint.
1.	1)	    Color: As Indicated in Drawings.
2.	2)	    Color: As Selected by Architect.
3.	3)	    Color: ______.
1.	5.		Panels:
a.	a.		1/8” Aluminum Panel.
b.	b.		Text and Graphics: As indicated on Drawings.
c.	c.	     Text and Graphics: As Selected by Architect.
d.	d.		Size: As indicated on Drawings.
A.	B.	    H2.2 Series Post and Panel Signage System
1.	1.	     Model No: As indicated on Drawings.
2.	2.	     Model No: As selected by Architect.
3.	3.	     Model No: (Follow naming convention as described in catalog). H2.2 - Post Type- Body Type - Panel Type - Sign Type - Graphic Process – Height – Width.
a.	a.	    	Description:  Non-illuminated Post and panel signage using Aluminum posts with two layers of panels of either Dibond or Aluminum; Can be constructed with different frames (body) for the panels and either 0 inch, 3/8 inch or 3/4 inch reveal.
b.	b.	     Size: As indicated on Drawings.
c.	c.	     Size: As selected by Architect.
d.	d.	     Size: __ inches (__ mm) in height  x __inches (__ mm) in width.
1.	4.		Posts:  Aluminum
a.	a.		2 inch (51 mm) square posts, 
b.	b.	     Length/Height:  As Indicated on Drawings.
c.	c.	     Length/Height:  As Selected by Architect.
d.	d.	     Length/Height:  ____ inches.
e.	e.	     Finish:  Paint.
1.	1)	     Color: As Indicated in Drawings.
2.	2)	     Color: As Selected by Architect.
3.	3)	     Color: ______.
1.	5.		Body Type (Select One)
a.	a.	     Slide Body: Framing Component to attach panels to posts showing a ½ inch frame at end of panels
b.	b.	     Bleed Body: Framing Component to attach panels to posts providing an edgeless appearance.
c.	c.	     Beveled Frame:  Framing Component to attach panels to posts providing a beveled frame around panels
1.	6.	     Reveal Size: As Selected by Architect.
2.	7.	     Reveal Size: 0 inch.
3.	8.	     Reveal Size: 3/8 inch.
4.	9.	     Reveal Size: 3/4 inch.
5.	10.	    Panels:
1.	1)	1/8 inch Aluminum Panel
2.	2)	1/8 inch Dibond Panel.
3.	3)	Text and Graphics: As indicated on Drawings.
4.	4)	Text and Graphics: As Selected by Architect.
5.	5)	Size: As indicated on Drawings.
6.	6)	Size: As selected by Architect.
7.	7)	Size: __ inches (__ mm) in height  x __inches (__ mm) in width.
3.	3.	   	H2.3 Series Post and Panel Signage System
a.	a.		Model No: As indicated on Drawings; 
b.	b.	     Model No: As selected by Architect; 
c.	c.	     Model No: (Follow naming convention as described in catalog). H2.3 - Post Type- Body Type - Panel Type - Sign Type - Graphic Process – Height - Width}.
1.	1)	Description:  Non-illuminated Post and panel signage using Aluminum posts with two layers of panels of either Dibond or Aluminum; can be constructed with different frames (body) for the panels and either 0 inch, 3/8 inch or 3/4 inch reveal.
2.	2)	Size: As indicated on Drawings.
3.	3)	Size: As selected by Architect.
4.	4)	Size: __ inches (__ mm) in height  x __inches (__ mm) in width.
d.	d.		Posts:  Aluminum
1.	1)	3 ¼ inch (83 mm) square posts
2.	2)	3 ¼ inch (83 mm) square posts with radius edges
3.	3)	3 ¼ inch (83 mm) rectangular posts
4.	4)	3 ¼ inch (83 mm) rectangular posts with radius edges
5.	5)	3 ¼ inch (83 mm) triangular posts
6.	6)	3 ¼ inch (83 mm) triangular posts with radius edges
7.	7)	3 ¼ inch (83 mm) diameter round post
8.	8)	3 ¼ inch (83 mm) diameter half round post
9.	9)	Shape as Indicated on Drawings
10.	10)	Shape as Selected by Architect.
11.	11)	Length/Height: As Indicated on Drawings.
12.	12)	Length/Height: As Selected by Architect.
13.	13)	Length/Height: ____ inches.
14.	14)	Finish:  Paint
a.	a)	    Color: As Indicated in Drawings.
b.	b)	    Color: As Selected by Architect.
c.	c)	    Color: ______.
a.	e.	     Body Type (Select One)
1.	1)	Slide Body: Framing Component to attach panels to posts showing a ½ inch frame at end of panels
2.	2)	Bleed Body: Framing Component to attach panels to posts providing an edgeless look.
3.	3)	Round Body:  Framing Component to attach panels to posts providing a rounded edge to end of panels
a.	f.	     Reveal Size: As Indicated on Drawings.
b.	g.	     Reveal Size: As Selected by Architect.
c.	h.	     Reveal Size: 0 inch.
d.	i.	     Reveal Size: 3/8 inch.
e.	j.	     Reveal Size: 3/4 inch.
f.	k.	     Panels:
1.	1)	1/8 inch Aluminum Panel
2.	2)	1/8 inch Dibond Panel
3.	3)	Text and Graphics: As indicated on Drawings.
4.	4)	Text and Graphics: As Selected by Architect.
5.	5)	Size: As indicated on Drawings.
6.	6)	Size: As selected by Architect.
7.	7)	Size: __ inches (__ mm) in height x __inches (__ mm) in width.
3.	4.	     RG130 (RG) Series Engineered Post and Panel Signage System:  As manufactured by Corpus Christi Stamp Works Inc. DBA/ National Signage Affiliates 
a.	a.	Model No: As indicated on Drawings.
b.	b.	Model No: As selected by Architect.
c.	c.	Model No: (Follow naming convention as described in catalog). RG - Post Type- Body Type - Panel Type - Sign Type - Graphic Process – Height - Width.
1.	1)	Description:  Non-illuminated Post and panel signage using Aluminum posts with Aluminum panels engineered to withstand wind speeds up to 130 mph.
2.	2)	Size: As indicated on Drawings; 
3.	3)	Size: As selected by Architect; 
4.	4)	Size: __ inches (__ mm) in height  x __inches (__ mm) in width}
a.	d.	Posts:
1.	1)		6061-T6 Aluminum extrusion with Mill Finish in accordance with ASTM-B209
2.	2)	     Square shape
3.	3)	     Thickness:  Per Engineer’s specification
4.	4)	     Wall Thickness:  Per Engineer’s specification  
5.	5)	     Length/Height:  As Indicated on Drawings; 
6.	6)	     Length/Height:  ____ inches.
7.	7)	     Finish:  Paint
a.	a)	    Color: As Indicated in Drawings; 
b.	b)	    Color: As Selected by Architect; 
c.	c)	    Color:  ______.
a.	e.	Panels:
1.	1)		1/4 inch 6061-T6 Aluminum panel with Mill Finish in accordance with ASTM-B209 or in a thickness as specified by the Engineer.
2.	2)		Text and Graphics: {As indicated on Drawings; As Selected by Architect}
3.	3)		Size: As indicated on Drawings
a.	f.	Hardware:
1.	1)	Hardware to be countersunk stainless steel.
2.	2)	Paint or otherwise protect the metal components from galvanic action according to Engineer’s instructions.
3.	3)	Size: Per Engineer’s specification
a.	g.	Footing:
1.	1)	Construct footings for signage per Engineer specification or as indicated on Drawings.
** NOTE TO SPECIFIER ** Delete if not required. 	
A.	C.	     Exterior Traffic Signs: As manufactured by Corpus Christi Stamp Works Inc. DBA/ National Signage Affiliates.
1.	1.		Material: .080 inch (2 mm) Aluminum.
** NOTE TO SPECIFIER ** Delete options for graphics not required. 
1.	2.		Graphics: As indicated on Drawings.
2.	3.		Graphics: As selected by Architect.
3.	4.		Graphics: ' One Way'.
4.	5.		Graphics: ' Do Not Enter'.
5.	6.		Graphics: ' Reserved Parking' with handicap symbol.
6.	7.		Graphics: ' Stop'.
7.	8.		Graphics: Pedestrian symbol.
8.	9.		Graphics: ' One Way'.
2.	2.4 		GRAPHIC APPLICATION METHODS
** NOTE TO SPECIFIER ** Delete options not required. 
A.	A.		GP-1 Engraved.
1.	1.		Process: Engraved, incised letter or image, paint-filled for non-ADA applications.  
2.	2.	     Color: As Indicated on Drawings.
3.	3.	     Color: As Selected by Architect; 
4.	4.	   Color: ________.
** NOTE TO SPECIFIER ** Delete options for materials not required. 
1.	5.		Materials: As indicated on Drawings.
2.	6.		Materials: As selected by Architect.
3.	7.		Materials: Laminate.
4.	8.		Materials: Acrylic.
5.	9.		Materials: Aluminum.
6.	10.		Materials: Brass.
7.	11.		Materials: Bronze.
8.	12.		Materials: Corian.
** NOTE TO SPECIFIER ** Manufacturing Process ADA approved. Delete if not required. 
A.	B.		GP-3 Subsurface Graphic Application:
1.	1.		Description: Process in which an image is reversed on the background surface. A background color is then applied for contrast, giving it a subsurface effect. This process is impervious to weather and easily maintained.
2.	2.		Material: Clear non-glare acrylic.
** NOTE TO SPECIFIER ** Delete options for thickness not required. 
1.	3.		Thickness: As indicated on Drawings.
2.	4.		Thickness: As selected by Architect.
3.	5.		Thickness: .060 inch (1.5 mm).
4.	6.		Thickness: .080 inch (2 mm).
5.	7.		Thickness: .125 inch (3 mm).
** NOTE TO SPECIFIER ** Delete if not required. 
A.	C.		GP-4 Vinyl: 
1.	1.		Description: Vinyl legends and text computer generated from 3 mil pressure sensitive material prepared for application to any smooth, non-porous surface.
** NOTE TO SPECIFIER ** Delete if not required. 
A.	D.		GP-5 Gemini: ADA compliant(Exterior Use).
1.	1.		Description: Precision cut letter raised 1/32 inch (0.8 mm) and chemically welded to subsurface acrylic in the following thicknesses: .060 inch (1.5 mm), .125 inch (3 mm), .015 (0.4 mm) vinyl laminates to 
2.	2.		Material: .125 inch (3 mm) black acrylic.
** NOTE TO SPECIFIER ** Delete options for thickness not required. 
1.	3.		Thickness: As indicated on Drawings.
2.	4.		Thickness: As selected by Architect.
3.	5.		Thickness: .015 inch (0.4 mm).
4.	6.		Thickness: .060 inch (1.5 mm).
5.	7.		Thickness: .125 inch (3 mm).\
F.	F.		GP6 - Digital Print
1.	1.	Description: Printing from a digital based image directly to paper or vinyl
1.	PART  3	  EXECUTION
2.	3.1 		EXAMINATION
A.	A.		Installer shall examine signs for defects, damage, and compliance with specifications.  Installation shall not proceed until satisfactory conditions are achieved.
B.	B.	    Inspect conditions of substrate and other conditions which may affect installation of signage. 
C.	C.		Do not begin installation until substrates are within manufacturer's specified tolerances and have been prepared in accordance with manufacturer's instructions.
D.	D.		If substrate preparation is the responsibility of another installer, do not proceed with installation. Notify Architect of any unsatisfactory conditions immediately. 
E.	E.		Commencement of work is deemed as acceptance of installation conditions.
3.	3.2 		PREPARATION
A.	A.		Verify mounting heights and locations for signage will comply with specified requirements, including accessibility requirements.
B.	B.		Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions. Clean mounting locations of dirt, dust, grease or similar conditions that would prevent proper installation.
4.	3.3 		INSTALLATION
A.	A.		Install in accordance with manufacturer's printed installation instructions, and in proper relationship with adjacent work.
B.	B.	  Use mounting methods and fasteners as recommended by the manufacturer.
C.	C.	  Set level, plumb, rigid and at heights indicated with surfaces free from defects.
5.	3.4 		PROTECTION
A.	A.		Protect installed products until completion of project.
B.	B.		Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION